# Cloud Service - Monitoring Parameters

Here you will find detailed information about monitoring parameters for Cloud monitored objects.

Monitoring parameters are the mechanism for you to configure how your systems are monitored. They are how you set configuration of how the agent runs, how checks are executed, thresholds for checks (when does a check go critical or warning) and much more. All Monitoring Parameters have a carefully chosen default value. As soon as you add a new system, Avantra uses these defaults. You may change these defaults by defining a parameter and by modifying its values. Monitoring Parameters can be defined for a single system, or for collections of systems using Monitoring Parameter Sets. You can also define your own Custom Monitoring Parameters for use within Custom Checks and automations.

## CPI_CUMapExpirationThreshold

Description

This monitoring parameter defines the expiration period for the CPI_CertificateUserMappingExpiration check. The threshold for highlighting if a certificate as due to expire is defined as today plus the number of days set in the monitoring parameter.

Reference Data

Configures | CPI_CertificateUserMappingExpiration
Default Value | 120
Unit | Days

## CPI_KeystoresExpirationThreshold

Description

Monitoring parameter CPI_KeystoresExpirationThreshold defines the expiration period for the CPI_KeystoreExpiration check. The threshold for highlighting if a certificate as due to expire is defined as today plus the number of days set in the monitoring parameter.

Reference Data

Configures | CPI_KeystoreExpiration
Default Value | 120
Unit | Days

## CPI_MessageLogCheckDays

Description

This monitoring parameter defines the check period for CPI_MessageLogs check. The period is the number of days from today to check for failed message logs.

Reference Data

Configures | CPI_MessageLogs
Default Value | 21
Unit | Days

## SCCOpenConnectionsCountCrit

This monitoring parameter sets the critical threshold for the number of open connections to the SCC.

Reference Data

Configures | SCC_OpenConnections
Default Value | 200
Unit | Integer

## SCCOpenConnectionsCountWarn

This monitoring parameter sets the warning threshold for the number of open connections to the SCC. If the returned number of connections is between the SCCOpenConnectionsCountWarn and SCCOpenConnectionsCountCrit values, then the check result is Warning.

Reference Data

Configures | SCC_OpenConnections
Default Value | 100
Unit | Integer

## SCCSubaccountExclude

Description

This monitoring parameter gives the ability to exclude subaccounts in the SAP Cloud Connector (SCC) checks for more accurate monitoring. Any subaccount IDs in the monitoring parameter SCCSubaccountExclude are removed from the check. The IDs are excluded in CSV format, i.e., subaccountID1, subaccountID2.

Reference Data

Configures

  SCC_Subaccounts, SCC_TopTimeConsumers

Default Value
Unit

  String

## SCCTopTimeGlobalCrit

Description

This monitoring parameter defines the critical threshold for latency time in milliseconds.

Reference Data

Configures | SCC_TopTimeConsumers
Default Value | 500
Unit | Number

## SCCTopTimeGlobalWarn

Description

This monitoring parameter defines the warning threshold for latency time in milliseconds.

Reference Data

Configures | SCC_TopTimeConsumers
Default Value | 250
Unit | Number

## SCCTopTimeSpecificThresholds

Description

This monitoring parameter defines the specific critical thresholds for latency time in milliseconds. The data are entered in semicolon-comma separated list, e.g., `HTTP,resource1,10,20;HTTP,resource2,200,400`

Reference Data

Configures | SCC_TopTimeConsumers
Default Value Unit | String

## SCCMemoryHeapCrit

Description

This monitoring parameter defines the critical threshold for heap memory used, measured in percent.

Reference Data

Configures | SCC_MemoryStatus
Default Value | 80
Unit | PCT

## SCCMemoryHeapWarn

Description

This monitoring parameter defines the warning threshold for heap memory used, measured in percent.

Reference Data

Configures | SCC_MemoryStatus
Default Value | 70
Unit | PCT

## SCCMemoryPhysicalCrit

Description

This monitoring parameter defines the critical threshold for physical memory used, measured in percent.

Reference Data

Configures | SCC_MemoryStatus
Default Value | 80
Unit | PCT

## SCCMemoryPhysicalWarn

Description

This monitoring parameter defines the warning threshold for physical memory used, measured in percent.

Reference Data

Configures | SCC_MemoryStatus
Default Value | 70
Unit | PCT

## SCCMemoryVirtualCrit

Description

This monitoring parameter defines the critical threshold for virtual memory used, measured in percent.

Reference Data

Configures | SCC_MemoryStatus
Default Value | 80
Unit | PCT

## SCCMemoryVirtualWarn

Description

This monitoring parameter defines the warning threshold for virtual memory used, measured in percent.

Reference Data

Configures | SCC_MemoryStatus
Default Value | 70
Unit | PCT